## Connecting to the camera via USB

### Check the type of cable.

##### Use a USB Type-C cable.

- Use of genuine Canon products (Interface Cable IFC-100U or IFC-400U) is recommended.

### Check the USB settings on the camera.

##### Check the camera settings and make sure it is ready for USB connection.

1. Press the camera's [MENU] button to display the menu.

2. On the MENU screen, select [Choose USB connection app] on the tab below.

3. Select [Photo Import/Remote Control].

4. Connect the camera and smartphone with a cable.

#### MEMO

- If the camera is not recognized after switching the camera settings, turn the camera off and on again.

### Please review the app settings.

##### Depending on the model of your smartphone, you may be able to connect by changing the [Connection mode].

- Select [Connection mode] from the button in the upper right corner of the top screen and set [Prioritize connectivity with camera].

### Check your smartphone settings.

##### Depending on the model of your smartphone, you may need to enable the ability to communicate with devices connected via USB.

- The name of the function varies depending on the model of the smartphone, but if there is an item called [OTG], turn it on.